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	Item
	Quantity
	Designation
	Price/unit
EUR
	Total
EUR

	1
	
	Supplying and laying of: 
m²  roof panels RD___
Roof sandwich element consisting of an external and internal steel cover shell which are connected in a shear-resistant manner via a heat-insulating rigid polyurethane foam core (density of approx. 40kg/m³)
Requirement: approved by building authorities and quality-monitored
Construction material class: Euro class B-s2, d0 (flame retardant)
Element thickness: ___ mm (corresponds to ___ mm insulating core)
Heat transmission coefficient (u-value) certified to EN 14509 with joint: ______ W/m²(K (see data sheet PU insulating panel RD)
Effective width: 1000 mm
Interior/exterior finish:
Outer face: galvanized sheet steel 0.6 mm, ROMAplus 50µm, in standard RAL xxxx color tone; lined
Internal face: galvanized stainless steel 0.5 mm, DU paint finish 10 - 15 µm, similar to RAL 9002; lined
Laying of ready-to-assemble elements is carried out on steel profiles (secondary carriers) coated with rust protection.
Roof pitch: x degrees
Static system: Multi-span beam
Rib spacing: approx. x.00 m
Element length: up to x.00 m
Snow load:: x.x kN/m²
Rib construction: Steel beam or wood connector ribs
The roof elements must be fastened onto the ribs with rustproof fastening materials featuring a screw-type technology approved by the building authorities and in accordance with specialist rules of the lightweight metal construction federation IFBS (Industrieverband für Bausysteme im Metallleichtbau).
All required insulating and fastening materials must be included in the calculation. 
Model and type to be offered as described:
ROMA RD ___

	
	

	2
	
	m  shed roof end profile for roof element
Supplying and installing polyester-coated shed roof end profile in panel color, including  profile filler, sealing tapes, cog sheeting, fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: approx. 600 mm
Bends: 6
	
	

	3
	
	m  ridge cover for roof element
Supply and install ridge cover, polyester-coated inside and outside, in panel color,
The price includes:
Ridge flashing inside and outside, filler pieces, profile filler, sealing tapes, cog sheeting, foam filling, including fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: Ridge flashing inside and outside approx. 600 mm each
Bends: approx. 3 each
	
	

	4
	
	m  verge profile for roof element
Supplying and installing polyester-coated verge profile in panel color, including  fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: approx. 550 mm
Bends: 7
	
	

	5
	
	m  wall connection on top shed roof side
Supply and install polyester-coated wall connection profile and inside corner trim in panel color.
The price includes:
Wall connection profile, inside corner trim, bending open the bottom edge of corrugated profile on the outer cover shell, filler pieces, profile fillers, sealing tapes, cogged sheeting, foam filling, including sealing to wall surface, fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: Wall connection approx. 450 mm, angle profile approx. 200 mm
Bends: 4 or 3
	
	

	6
	
	m  side wall connection profile
Supply and install polyester-coated wall connection profile and inside corner trim in panel color.
The price includes:
Wall connection profile, inside cover trim, filler pieces, sealing tapes, foam filling including sealing wall surface, fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: approx. 450 mm, angle profile approx. 200 mm
Bends: 5 or 3
	
	

	7
	
	m  water deflector plate for roof element
Supplying and installing polyester-coated water deflector plate in panel color, including  fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: approx. 300 mm
Bends: 3

	
	

	8
	
	m  gutter inflow sheet for roof element
Supplying and installing polyester-coated water deflector plate in panel color, including  sealing tape, fastening materials and trimming 
Sheet thickness:  0.75 mm
Layout: approx. 250 mm
Bends: 2
	
	

	9
	
	m box gutter 
Supplying and installing box gutter with nominal size of xxx mm, bracket-mounted, matching panel system, including all bends, drains, fastenings, gutter brackets and end pieces.
Drain openings: x pcs
Expansion joints are to be included if necessary
	
	

	10
	
	m end lap formation
Create an overlap of the element faceplates via a foam-free cutback, including required sealing tapes and connection elements in compliance with specialist IFBS rules
	
	

	11
	
	m cladding profile (apron plate)
From the roof ridge as a connection plate to the roof openings for ventilation pipes, chimney, other openings, etc.
Supplying and installing polyester-coated cladding profile in panel color, including  required sealing tapes and fastening material
The hollow space between the roof element and cladding profile must be completely closed off using suitable insulating material.
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